**How to Run RITG148+**

**Purpose:** This procedure explains how to begin using RITG148+ film analysis software. It assumes that the program has been installed on the computer on which you wish to use it. If RITG148+ has not been installed, see the *RITG148+ Software Manual*.

**Before first-time use:**

Set the program to run in Windows 8 compatibility mode. This must be done for each user account, as setting it globally requires admin rights.

1. Navigate to **C:\RIT\RIT113V4**.
2. Do the following for each of **Rit Launcher** and **RIT113V4**:
   1. Right-click and select **Properties**.
   2. On the **Compatibility** tab, check **Run this program in compatibility mode for:** and select **Windows 8** from the dropdown list.
   3. Click **OK**.

**Film analysis with VIDAR scanner:**

Page 13 of the *RITG148+ Software Manua*l describes how to export a VIDAR scan as a TIFF file. A couple things to keep in mind:

1. Plug in the VIDAR scanner to the computer.
2. Start RITG148+ and wait ~20–90 minutes for the scanner to ready itself and for the RITG148+ “Loading” message to disappear.
3. Click **Launch** in the RITG148+ window.
4. See page 13 of the *RITG148+ Software Manual* for instructions on exporting the scan as a TIFF file.