How to Run RITG148+

# Purpose

This procedure explains how to begin using RITG148+ film analysis software. It assumes that the program has been installed on the computer on which you wish to use it. If RITG148+ has not been installed, see the *RITG148+ Software Manual*.

# At login

Set the program to run in Windows 8 compatibility mode. This must be done for each user account, as setting it globally requires admin rights. It also resets at logout, so you must do it again every time you log in.

1. Navigate to **C:\RIT\RIT113V4**.
2. Do the following for each of **Rit Launcher** and **RIT113V4**:
   1. Right-click and select **Properties**.
   2. On the **Compatibility** tab, check **Run this program in compatibility mode for:** and select **Windows 8** from the dropdown list.
   3. Click **OK**.

# Film analysis with VIDAR scanner

Page 13 of the *RITG148+ Software Manua*l describes how to export a VIDAR scan as a TIFF file. A couple things to keep in mind:

1. Plug in the VIDAR scanner to the computer.
2. Start RITG148+ and wait ~20–90 minutes for the scanner to ready itself and for the RITG148+ “Loading” message to disappear.
3. Click **Launch** in the RITG148+ window.
4. See page 13 of the *RITG148+ Software Manual* for instructions on exporting the scan as a TIFF file.