Adjust Elekta Lasers

1. Get laser remote hand pendant.
2. Note number of lasers (on bottom front of case) to adjust.
3. Turn on lasers.
4. Point laser remote hand pendant toward laser to be adjusted.
5. On laser remote hand pendant, press *SELECT* > *SELECT*.
6. For each laser that needs to be adjusted:
   1. Press *#* and enter the laser number (1–4). The selected laser will blink, and the green light on the front bottom of the case will glow brightly.
   2. Adjust the selected laser using the button in the middle of the laser remote hand pendant.
   3. The laser will be deselected when no adjustments have been made for a couple minutes.